
1. Put the server(your computer) and phone in the same hub(or at same lan network ),or contact the computer with lan port of phone.
2. Make the Phone enter post mode: power off🡪 long press “#”🡪power on ,Release # button until phone UI shows post mode.
3. Set the ip of computer to 192.168.10.99
4. Open ftp server, add a user, the username and password is: username/userpasswd



1. Open the computer's Command Prompt window,
2. telnet 192.168.10.1
3. Enter u
4. Enter voipwl
5. The flashfile.bin will upload to ftp download directory

